* Port 1 header pin 4 labeled incorrectly (should be 6)
* Opamp pins connected wrong. Error with device definitions.
* Increase size of terminal blocks for wire gauge suited for amperage specs
* Voltage regulator doesn’t work
* Different resistor values